IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Número de proyecto"
Time stamp: "2016-09-05T15:48:29"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140223_1515(x64) - Exporter 15.6.0.0 - Alternate UI 15.6.0.0"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "tobal_000" of Organization (no name given)
  Owner history of Person "tobal_000" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Número de proyecto" | long name "Nombre de proyecto" | phase "Estado de proyecto"
  IFCSITE "Default" | latitude 40° 25′ 0.086975″ | longitude -3° 42′ 1.243858″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Introduzca dirección aquí", "Madrid", "España"
      IFCBUILDINGSTOREY "Nivel 1" | long name "Nivel 1" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1230x1480 mm Corredera" | object type "1230x1480 mm Corredera" | names: "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas:1230x1480 mm Corredera:152403" | material: materials ("Cristal - Vidrio claro templado", "Aluminio") | property sets: Pset_WindowCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Other

Types
  IFCWINDOWSTYLE "1230x1480 mm Corredera" | 1 occurrence | material: materials ("Cristal - Vidrio claro templado", "Aluminio") | property sets: 2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas:1230x1480 mm Corredera:152403, Analysis Results, Analytical Properties, Construction, Data, Dimensions

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Propietario" (IFCTEXT)
    Project Address = "Introduzca dirección aquí" (IFCTEXT)
    Project Issue Date = "Fecha de emisión" (IFCTEXT)
    Project Name = "Nombre de proyecto" (IFCTEXT)
    Project Number = "Número de proyecto" (IFCTEXT)
    Project Status = "Estado de proyecto" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas: 1230x1480 mm Corredera" (IFCLABEL)
    Family and Type = "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas: 1230x1480 mm Corredera" (IFCLABEL)
    Head Height = 2.28 (IFCLENGTHMEASURE) [METRE]
    Host Id = "Basic Wall: Por defecto - 30 cm" (IFCLABEL)
    Type = "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas: 1230x1480 mm Corredera" (IFCLABEL)
    Type Id = "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas: 1230x1480 mm Corredera" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Nivel 1" (IFCLABEL)
    Family and Type = "Level: Nivel 1" (IFCLABEL)
    Type = "Level: Nivel 1" (IFCLABEL)
    Type Id = "Level: Nivel 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas" (IFCTEXT)
    InstruccionesEspeciales = "" (IFCTEXT)
    MaterialContenedor = "" (IFCTEXT)
    MaterialEnvase = "" (IFCTEXT)
    TipoEmbalajeProteccion = "" (IFCTEXT)
    a = 3391003.112 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1230x1480 mm Corredera" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCWINDOW)
    Manufacturer = "Grupo ALUGOM" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Level = "Level: Nivel 1" (IFCLABEL)
    Sill Height = 0.799999999999999 (IFCLENGTHMEASURE) [METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Area = 4.1268399449116 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.08741017646444 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [METRE]
  Dimensions | properties | on 1 type object
    Altura Máxima = 2.5 (IFCLENGTHMEASURE) [METRE]
    Altura Real = 1.48 (IFCLENGTHMEASURE) [METRE]
    AnchoMarco = 0.147 (IFCLENGTHMEASURE) [METRE]
    AnchoMarcoCentral = 0.108 (IFCLENGTHMEASURE) [METRE]
    Anchura Máxima = 4. (IFCLENGTHMEASURE) [METRE]
    Anchura Real = 1.23 (IFCLENGTHMEASURE) [METRE]
    DesfaseExterior = 0. (IFCLENGTHMEASURE) [METRE]
    DesfaseInterior = 0. (IFCLENGTHMEASURE) [METRE]
    GrosorAcristalamiento = 0.022 (IFCLENGTHMEASURE) [METRE]
    GrosorMarco = 0.135 (IFCLENGTHMEASURE) [METRE]
    Height = 1.48 (IFCLENGTHMEASURE) [METRE]
    Perimetro = 5420. (IFCREAL)
    Width = 1.23 (IFCLENGTHMEASURE) [METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Nivel 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Nivel 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Autor = "Bimetica Parametric Design Services, S.L." (IFCTEXT)
    AñoProduccion = "" (IFCTEXT)
    Bimetica = "http://www.bimetica.com" (IFCTEXT)
    COBieCategoria = "" (IFCTEXT)
    CodigoBarras = "" (IFCTEXT)
    CondicionesGeneralesDeContratacion = "" (IFCTEXT)
    ContenidoGarantia = "" (IFCTEXT)
    Description = "Ventana Corredera" (IFCTEXT)
    DuracionVidaUtil = "" (IFCTEXT)
    EmailContacto = "alugom@alugom.com" (IFCTEXT)
    EtiquetaModelo = "" (IFCTEXT)
    Exclusiones = "" (IFCTEXT)
    FechaCompra = "" (IFCTEXT)
    FechaEmisionElementoBIM = "01/09/2016" (IFCTEXT)
    FechaFinGarantia = "" (IFCTEXT)
    FechaInicioGarantia = "" (IFCTEXT)
    FechaVencimientoElementoBIM = "01/09/2017" (IFCTEXT)
    GarantiaExtendida = "" (IFCTEXT)
    IFCClasificacion = "" (IFCTEXT)
    IdentificadorGarantia = "" (IFCTEXT)
    InformacionTecnica = "" (IFCTEXT)
    LugarEnsamblaje = "" (IFCTEXT)
    Manufacturer = "Grupo ALUGOM" (IFCTEXT)
    MasterformatCodigo = "08 51 13" (IFCTEXT)
    MasterformatTitulo = "Aluminum Windows" (IFCTEXT)
    Model = "Serie Martra 135RPT" (IFCTEXT)
    NumeroArticulo = "" (IFCTEXT)
    NumeroArticuloGlobalComercial = "" (IFCTEXT)
    NumeroSerie = "" (IFCTEXT)
    OmniClass Number = "23.30.20.00" (IFCTEXT)
    OmniClass Title = "Windows" (IFCTEXT)
    OmniclassCodigo = "23.30.20.17.14.14" (IFCTEXT)
    OmniclassTitulo = "Horizontal Sliding Windows" (IFCTEXT)
    PeriodoGarantia = "" (IFCTEXT)
    PuntoDeContacto = "" (IFCTEXT)
    Referencia = "" (IFCTEXT)
    ReferenciaContacto = "Alugom" (IFCTEXT)
    ReferenciaLote = "" (IFCTEXT)
    ResistenciaFuego = "" (IFCTEXT)
    TelefonoContacto = "+34 91 616 47 27" (IFCTEXT)
    TiempoMedioEntreFallos = "" (IFCTEXT)
    Type Comments = "Sistema de Ventana de 2 Hojas Rotura de Puente Térmico Serie Martra 135RPT Corredera" (IFCTEXT)
    Type Mark = "21" (IFCTEXT)
    Type Name = "1230x1480 mm Corredera" (IFCTEXT)
    UNSPSCCodigo = "30-17-16-07" (IFCTEXT)
    UNSPSCTitulo = "Horizontal slider windows" (IFCTEXT)
    URLProducto = "" (IFCTEXT)
    Uniclass2.0Codigo = "30-00-00" (IFCTEXT)
    Uniclass2.0Titulo = "Accessible openings: Doors and hatches, French windows, sliding wall windows." (IFCTEXT)
    VersionElementoBIM = "1.0" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCWINDOW)
    Phase Created = "Nueva construcción" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCWINDOW)
    Aperturas = TRUE (IFCBOOLEAN)
    Aperturas Oscilobatiente = FALSE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    Corredera = TRUE (IFCBOOLEAN)
    Detalle Perfileria = TRUE (IFCBOOLEAN)
    Manija = TRUE (IFCBOOLEAN)
    Oscilobatiente = FALSE (IFCBOOLEAN)
    Practicable = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Trazo punto" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Extremo de nivel: Extremo de nivel" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  2015_Ventana_Alugom_Matra-135RPT_Corredera-2-Hojas:1230x1480 mm Corredera:152403 | predefined | on 1 type object
  Analysis Results | properties | on 1 type object
    FactorSolarModificado = 30000000. (IFCREAL)
    FactorSombra = 0. (IFCREAL)
    FraccionAreaAcristalamiento = 0.539446275543837 (IFCREAL)
    Y𝑔 P1 = 0.47 (IFCREAL)
    Y𝑔 P2 = 0.47 (IFCREAL)
    𝐴𝑓 P1 = 710304. (IFCREAL)
    𝐴𝑓 P2 = 128088. (IFCREAL)
    𝐴𝑔 V1 = 491004. (IFCREAL)
    𝐴𝑔 V2 = 491004. (IFCREAL)
    𝑈𝑓 P1 = 2.42 (IFCREAL)
    𝑈𝑓 P2 = 3.039 (IFCREAL)
    𝑈𝑔 V1 = 1. (IFCREAL)
    𝑈𝑔 V2 = 1. (IFCREAL)
    𝑈𝑤 = 1.86277912107229 (IFCREAL)
    𝑙𝑔 P1 = 4028. (IFCREAL)
    𝑙𝑔 P2 = 2372. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
  Construction | properties | on 1 type object
    Altura de antepecho por defecto = 0.799999999999999 (IFCLENGTHMEASURE) [METRE]
    CerramientoExterior = TRUE (IFCBOOLEAN)
    ConfiguracionPoliamidas = "215600 - 955100" (IFCTEXT)
    ControlHumos = FALSE (IFCBOOLEAN)
    Estado = "" (IFCTEXT)
    Motorizada = FALSE (IFCBOOLEAN)
    NivelSeguridad = "" (IFCTEXT)
    RepisaExterior = TRUE (IFCBOOLEAN)
    RepisaInterior = TRUE (IFCBOOLEAN)
    SalidaEmergencia = TRUE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Data | properties | on 1 type object
    Area = 1.8204 (IFCAREAMEASURE) [SQUARE_METRE]
    CondicionesEvaluacion = "" (IFCTEXT)
    DescripcionEvaluacion = "" (IFCTEXT)
    EstanqueidadAgua = "Clase 8A" (IFCTEXT)
    FechaEvaluacion = "" (IFCTEXT)
    IndiceGlobalRedAcustica = "" (IFCTEXT)
    IndiceGlobalRedAcusticaTr = "32 dBA" (IFCTEXT)
    MasaSuperficialKgm2 = 0. (IFCREAL)
    PermeabilidadAlAire = "Clase 3" (IFCTEXT)
    ResistenciaAlViento = "Clase C5" (IFCTEXT)
    TransmitanciaTermica = 3.7 (IFCREAL)
  General | properties | on 1 type object
    CertificadoMantenimiento = "" (IFCTEXT)
    CodigoBedec = "" (IFCTEXT)
    CondicionesMantenimiento = "" (IFCTEXT)
    CosteMantenimiento = 0. (IFCREAL)
    FechaInstalacion = "" (IFCTEXT)
    FrecuenciaMantenimiento = "" (IFCTEXT)
    MateriaPrima = 0. (IFCREAL)
    NormativaMantenimiento = "" (IFCTEXT)
    TrabajoMantenimiento = "" (IFCTEXT)
    UnidadMantenimiento = "" (IFCTEXT)
    UnidadMedicion = "" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    AcidificacionAtmosferica = 0. (IFCREAL)
    AcidificacionAtmosfericaPorUnidad = 0. (IFCREAL)
    AguaConsumida = 0. (IFCREAL)
    AguaConsumidaPorUnidad = 0. (IFCREAL)
    CambioClimatico = 0. (IFCREAL)
    CambioClimaticoPorUnidad = 0. (IFCREAL)
    CosteEnergeticoKwh = 0. (IFCREAL)
    CosteEnergeticoMj = 0. (IFCREAL)
    DestruccionCapaOzonoEstratosferica = 0. (IFCREAL)
    DestruccionCapaOzonoEstratosfericaPorUnidad = 0. (IFCREAL)
    EmisionCO2 = 0. (IFCREAL)
    EnergiaNoRenovableConsumida = 0. (IFCREAL)
    EnergiaNoRenovableConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaPrimariaTotalConsumida = 0. (IFCREAL)
    EnergiaPrimariaTotalConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaRenovableConsumida = 0. (IFCREAL)
    EnergiaRenovableConsumidaPorUnidad = 0. (IFCREAL)
    Eutrofizacion = 0. (IFCREAL)
    EutrofizacionPorUnidad = 0. (IFCREAL)
    FaltaDeRecursos = 0. (IFCREAL)
    FaltaDeRecursosPorUnidad = 0. (IFCREAL)
    FaseCicloVida = "" (IFCTEXT)
    FormacionFotoquimicaOzono = 0. (IFCREAL)
    FormacionFotoquimicaOzonoPorUnidad = 0. (IFCREAL)
    ReferenciaUnidadFuncional = "" (IFCTEXT)
    ResiduoInerte = 0. (IFCREAL)
    ResiduoInertePorUnidad = 0. (IFCREAL)
    ResiduoRadioactivo = 0. (IFCREAL)
    ResiduoRadioactivoPorUnidad = 0. (IFCREAL)
    ResiduosNoPeligrosos = 0. (IFCREAL)
    ResiduosNoPeligrososPorUnidad = 0. (IFCREAL)
    ResiduosPeligrosos = 0. (IFCREAL)
    ResiduosPeligrososPorUnidad = 0. (IFCREAL)
    Unidad = "" (IFCTEXT)
    VidaUtilEsperada = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Acabado = "" (IFCTEXT)
    Acristalamiento = "Cristal - Vidrio claro templado" (IFCLABEL)
    Marco = "Aluminio" (IFCLABEL)
    Poliamida = "Poliamida, Technoform Bautec, PA66 GF 25" (IFCLABEL)