IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2019-02-14T13:38:46"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "20181011_1500(x64) - Exporter 18.4.0.0 - ARCHICAD Connection 21.0.0.6007"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"
Application: "ARCHICAD Connection for Revit 2018" version "21.0.0" identifier "Add-in version: 6007 INT 64 bit" by Organization "GRAPHISOFT SE"

People and organizations
  Person "e.suszcz" of Organization (no name given)
  Owner history of Person "e.suszcz" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person "e.suszcz" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | created 0 (1970-01-01T00:00:00Z) | last modified with "ARCHICAD Connection for Revit 2018" version "21.0.0" identifier "Add-in version: 6007 INT 64 bit" by Organization "GRAPHISOFT SE"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCHEATEXCHANGERTYPE "ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" | object type "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin:ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" | names: "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin:ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm:359349" | material: materials ("RSen_x_rgb 255 255 255 T00 pure white_gen", "RSen_x_rgb 055 053 053 T00 gray_gen", "RSen_n6_PE_black") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCHEATEXCHANGERTYPE "ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" | PLATE | 1 occurrence | material: materials ("RSen_x_rgb 255 255 255 T00 pure white_gen", "RSen_x_rgb 055 053 053 T00 gray_gen", "RSen_n6_PE_black") | property sets: Constraints, Construction, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin:ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "Daikin Europe N.V." (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin:ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Reference Plane : h_leftright" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_accessory = "" (IFCTEXT)
    RSen_C_alignment = "Center" (IFCTEXT)
    RSen_C_alignment_index = 0 (IFCINTEGER)
    RSen_C_offset_from_base_level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_suspension_height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_GOg = FALSE (IFCBOOLEAN)
    TBQen_C_SOg = TRUE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RSen_C_accessory_index = 0 (IFCINTEGER)
    RSen_C_diameter_type = "OD" (IFCTEXT)
    RSen_C_diameter_type_index = 1 (IFCINTEGER)
    TBQen_C_SOg_01 = "standard" (IFCLABEL)
    TBQen_C_SOg_02 = "standard" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 84.0187272046 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 28.4038202639 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    RSen_C_diameter = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height = 1896. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 790. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 790. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_clearance_zone = FALSE (IFCBOOLEAN)
    RSen_C_connection_zone = FALSE (IFCBOOLEAN)
    RSen_C_maintenance_zone = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit_displacement_back = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_front = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_logo = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "24" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "56.10.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Air To Water Heat Pump" (IFCTEXT)
    Manufacturer = "Daikin Europe N.V." (IFCTEXT)
    Model = "Altherma" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    RSen_C_IFC_version = "2x3" (IFCTEXT)
    RSen_C_code_ETIM = "" (IFCTEXT)
    RSen_C_code_ETIM_URL = "" (IFCTEXT)
    RSen_C_code_article = "EHSX04P50DA" (IFCTEXT)
    RSen_C_code_gtin = "" (IFCTEXT)
    RSen_C_code_product = "EHSX04P50DA" (IFCTEXT)
    RSen_C_code_product_class = "EHSX-D" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "10/10/2018" (IFCTEXT)
    RSen_C_content_date_issue = "10/10/2018" (IFCTEXT)
    RSen_C_content_provider = "Daikin Europe N.V." (IFCTEXT)
    RSen_C_content_version = "1.0.0" (IFCTEXT)
    RSen_C_data_issue_date = "" (IFCTEXT)
    RSen_C_description = "Air To Water Heat Pump" (IFCTEXT)
    RSen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    RSen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    RSen_C_model = "Altherma" (IFCTEXT)
    RSen_C_revit_version = "2016" (IFCTEXT)
    RSen_C_type = "Heating, Cooling And Hot Water With Thermal Solar Support" (IFCTEXT)
    RSen_C_type_comments = "Floor Standing Indoor Unit" (IFCTEXT)
    TBQ_I BaseKeynote = "56.10.10" (IFCTEXT)
    Type Comments = "Floor Standing Indoor Unit" (IFCTEXT)
    Type Name = "ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCTEXT)
    URL = "www.daikineurope.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_P_c01_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c02_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c03_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c04_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c07_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c08_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Supply,Hydronic Return,Power,Controls,Hydronic Supply,Domestic Cold Water,Domestic Hot Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin: ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCLABEL)
    Family and Type = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin: ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCLABEL)
    Type = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin: ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCLABEL)
    Type Id = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin: ehsx04p50da - altherma_daikin_lxwxh 790x790x1896 mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "RSen_53_ME_FB_indoor unit - altherma - ehsh-ehsx-rhsx_daikin" (IFCTEXT)
    RSen_E_c01_description = "c01_el" (IFCTEXT)
    RSen_E_c01_power_factor_state = "Lagging" (IFCTEXT)
    RSen_E_c01_system_type = "Power - Balanced" (IFCTEXT)
    RSen_E_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_E_c02_description = "c02_controls" (IFCTEXT)
    RSen_E_c02_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c01_description = "c01_liquid connection" (IFCTEXT)
    RSen_P_c01_diameter = 6.4 (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_diameter_calc = 6.4 (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_flow_configuration = "Preset" (IFCTEXT)
    RSen_P_c01_flow_direction = "In" (IFCTEXT)
    RSen_P_c01_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c01_system_classification = "Hydronic Supply" (IFCTEXT)
    RSen_P_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c02_description = "c02_gas connection" (IFCTEXT)
    RSen_P_c02_diameter = 15.9 (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter_calc = 15.9 (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_flow_configuration = "Preset" (IFCTEXT)
    RSen_P_c02_flow_direction = "Out" (IFCTEXT)
    RSen_P_c02_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c02_system_classification = "Hydronic Return" (IFCTEXT)
    RSen_P_c02_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c03_description = "c03_heating return flow" (IFCTEXT)
    RSen_P_c03_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c03_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c03_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c03_flow_direction = "In" (IFCTEXT)
    RSen_P_c03_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c03_system_classification = "Hydronic Return" (IFCTEXT)
    RSen_P_c03_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c04_description = "c04_heating feed" (IFCTEXT)
    RSen_P_c04_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c04_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c04_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c04_flow_direction = "Out" (IFCTEXT)
    RSen_P_c04_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c04_system_classification = "Hydronic Supply" (IFCTEXT)
    RSen_P_c04_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c07_description = "c07_domestic hot water - cold water in" (IFCTEXT)
    RSen_P_c07_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c07_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c07_flow_configuration = "Preset" (IFCTEXT)
    RSen_P_c07_flow_direction = "In" (IFCTEXT)
    RSen_P_c07_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c07_system_classification = "Domestic Cold Water" (IFCTEXT)
    RSen_P_c07_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c08_description = "c08_domestic hot water - hot water out" (IFCTEXT)
    RSen_P_c08_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c08_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c08_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c08_flow_direction = "Out" (IFCTEXT)
    RSen_P_c08_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c08_system_classification = "Domestic Hot Water" (IFCTEXT)
    RSen_P_c08_yes_no = TRUE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_content_manual = "http://www.witas.be/en/daikin" (IFCTEXT)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 6 (IFCINTEGER)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 1 (IFCINTEGER)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 2 (IFCINTEGER)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 3 (IFCINTEGER)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 4 (IFCINTEGER)
  Pset_DistributionPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectionType = "WELDED" (IFCTEXT)
    PortNumber = 5 (IFCINTEGER)
  MEPPortPipe | properties | on 4 objects (4 IFCDISTRIBUTIONPORT)
    ConnectorDiameter = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalHeight = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalWidth = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    OuterDiameter = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    ProfileShape = "ROUND" (IFCTEXT)
  MEPPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectorDiameter = 6.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalHeight = 6.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalWidth = 6.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    OuterDiameter = 6.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    ProfileShape = "ROUND" (IFCTEXT)
  MEPPortPipe | properties | on 1 object (1 IFCDISTRIBUTIONPORT)
    ConnectorDiameter = 15.9 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalHeight = 15.9 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalWidth = 15.9 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    OuterDiameter = 15.9 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    ProfileShape = "ROUND" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  AC_Pset_RenovationAndPhasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Renovation Status = "New" (IFCLABEL)
  MEP_Proxy | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    MEP_InsShow = FALSE (IFCBOOLEAN)
    MEP_InsShow = FALSE (IFCBOOLEAN)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_division_engine = TRUE (IFCBOOLEAN)
    RSen_E_c01_load_class = "Other" (IFCLABEL)
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_power_factor = 1. (IFCREAL)
    RSen_E_c01_voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 255 255 255 T00 pure white_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Casing Colour = "Traffic white (RAL9016) / Dark grey (RAL7011)" (IFCTEXT)
    Casing Material = "Impact resistant polypropylene" (IFCTEXT)
    Control systems Infrared remote control = "No" (IFCTEXT)
    Control systems Wired remote control = "RoConPlus" (IFCTEXT)
    Dimensions Unit Height/Width/Depth mm = "1896 /790 /790 mm" (IFCTEXT)
    Electric heater Power supply Phase/Voltage/Frequency/Fuse = "1~/3~/50 Hz/" (IFCTEXT)
    Electrical power consumption Max. W = "62 W" (IFCTEXT)
    Electrical power consumption Standby W = "11 W" (IFCTEXT)
    IP class IP = "IP 40" (IFCTEXT)
    Installation Manual = "http://www.daikineurope.com/support-and-manuals/product-information/index.jsp?searchterm=EHSX04P50DA&searchcategory=product-information" (IFCTEXT)
    Operation range Cooling Water side Min./Max. °C = "5/22 °C" (IFCTEXT)
    Operation range Domestic hot water Water side Min./Max. °C = "25/55 °C" (IFCTEXT)
    Operation range Heating Ambient Min./Max. °C = "-" (IFCTEXT)
    Operation range Heating Water side Min./Max. °C = "18/65 °C" (IFCTEXT)
    Outdoor unit = "ERGA04DAV3/ERGA04DAV3A" (IFCTEXT)
    Piping connections Pressurised solar heat exchanger inch = "-" (IFCTEXT)
    Power input Nom. kW = "-" (IFCTEXT)
    Power supply Phase/Voltage/Frequency = "1~/230 V/50 Hz" (IFCTEXT)
    Refrigerant Charge kg = "1,50 kg" (IFCTEXT)
    Refrigerant Type = "R-32" (IFCTEXT)
    Refrigerant circuit Gas side diameter mm = "15,9 mm" (IFCTEXT)
    Refrigerant circuit Liquid side diameter mm = "6,35 mm" (IFCTEXT)
    Sound power level Nom. dBA = "39 dBA" (IFCTEXT)
    Sound pressure level Nom. dBA = "-" (IFCTEXT)
    Specification Text = "https://my.daikin.eu/denv/en_US/home/applications/asset-finder.html##%3Fi=1%3Bq4=document-language%253Aen%7Cdocument-language%253Anone%3Bq5=document-type%253Aspecification-text%3Bsort=date%3Bsp_d=specific%3Bsp_start_day=1%3Bsp_start_month=1%3Bsp_start_year=2011%3Btemplate=json%3Bx3=market%3Bx4=document-language%3Bx5=document-type%3Bq=EHSX04P50DA%3B" (IFCTEXT)
    Tank Corrosion protection = "-" (IFCTEXT)
    Tank Energy efficiency class = "B" (IFCTEXT)
    Tank Insulation Heat loss kWh/24h = "1,7 (1) kWh/24h" (IFCTEXT)
    Tank Insulation Material = "HFC-free Polyurethane foam" (IFCTEXT)
    Tank Material = "Polypropylen" (IFCTEXT)
    Tank Maximum water pressure bar = "-" (IFCTEXT)
    Tank Maximum water temperature °C = "85,0 (0,000) °C" (IFCTEXT)
    Tank Standing heat loss W = "72 W" (IFCTEXT)
    Tank Storage volume l = "477 l" (IFCTEXT)
    Water circuit - Domestic hot water side Piping connections Cold water in / Hot water out inch = "G 1" (male) inch" (IFCTEXT)
    Water circuit - Domestic hot water side Piping connections Recirculation connection inch = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Air purge valve = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Drain valve / fill valve = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Manometer = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Piping connections diameter inch = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Safety valve bar = "-" (IFCTEXT)
    Water circuit - space heating side (additional zone) Shut off valve = "-" (IFCTEXT)
    Water circuit - space heating side (main zone) Air purge valve = "Yes" (IFCTEXT)
    Water circuit - space heating side (main zone) Drain valve / fill valve = "Yes" (IFCTEXT)
    Water circuit - space heating side (main zone) Manometer = "Yes" (IFCTEXT)
    Water circuit - space heating side (main zone) Piping connections diameter inch = "G 1 (FEMALE) inch" (IFCTEXT)
    Water circuit - space heating side (main zone) Safety valve bar = "Yes bar" (IFCTEXT)
    Water circuit - space heating side (main zone) Shut off valve = "Yes" (IFCTEXT)
    Water circuit Piping connections diameter inch = "G 1" (male) inch" (IFCTEXT)
    Water circuit Piping inch = "-" (IFCTEXT)
    Water circuit Safety valve bar = "3 bar" (IFCTEXT)
    Weight Unit kg = "93,0 kg" (IFCTEXT)
    Wiring connections Communication cable Quantity = "-" (IFCTEXT)
    Wiring connections Communication cable Remark = "-" (IFCTEXT)
    Wiring connections Domestic hot water pump Quantity = "-" (IFCTEXT)
    Wiring connections Domestic hot water pump Remark = "-" (IFCTEXT)

Other addresses and roles
  2 x postal address: "## Street City, State Zip", "Boston", "MA"