IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2018-10-17T16:47:13"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20161004_0715(x64) - Exporter 16.0.1185.0 - Default UI"
Application: "Autodesk Revit MEP 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit MEP 2016 (ENU)"

People and organizations
  Person "e.suszcz" of Organization (no name given)
  Owner history of Person "e.suszcz" of Organization (no name given) | application "Autodesk Revit MEP 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit MEP 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "X:\ZZ\01\RSen_55_ME_FB_outdoor unit - altherma_daikin_ifc\RSen_55_ME_FB_outdoor unit - altherma_daikin_eblq011cav3 - altherma monobloc_daikin_eblq.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "eblq011cav3 - altherma monobloc_daikin_eblq" | object type "eblq011cav3 - altherma monobloc_daikin_eblq" | names: "RSen_55_ME_FB_outdoor unit - altherma_daikin:eblq011cav3 - altherma monobloc_daikin_eblq:5153008" | material: materials ("RSen_x_rgb 189 187 185 T80 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Construction, Dimensions, Electrical - Loads
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standard" | object type "standard" | names: "RSen_55_GM_FB_logo outdoor unit - SH_daikin:standard:5153009" | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen") | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing

Types
  IFCUNITARYEQUIPMENTTYPE "eblq011cav3 - altherma monobloc_daikin_eblq" | AIRCONDITIONINGUNIT | 1 occurrence | material: materials ("RSen_x_rgb 189 187 185 T80 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Constraints, Construction, Dimensions, Electrical, Electrical - Loads, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "standard" | 1 occurrence | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "RSen_55_ME_FB_outdoor unit - altherma_daikin: eblq011cav3 - altherma monobloc_daikin_eblq" (IFCLABEL)
    Family and Type = "RSen_55_ME_FB_outdoor unit - altherma_daikin: eblq011cav3 - altherma monobloc_daikin_eblq" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
    Type = "RSen_55_ME_FB_outdoor unit - altherma_daikin: eblq011cav3 - altherma monobloc_daikin_eblq" (IFCLABEL)
    Type Id = "RSen_55_ME_FB_outdoor unit - altherma_daikin: eblq011cav3 - altherma monobloc_daikin_eblq" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Family and Type = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Type = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Type Id = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "RSen_55_ME_FB_outdoor unit - altherma_daikin" (IFCTEXT)
    RSen_E_c01_description = "c01_el" (IFCTEXT)
    RSen_E_c01_power_factor_state = "Lagging" (IFCTEXT)
    RSen_E_c01_system_type = "Power - Unbalanced" (IFCTEXT)
    RSen_E_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_E_c02_description = "c02_controls" (IFCTEXT)
    RSen_E_c02_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c01_description = "c01_water out connection" (IFCTEXT)
    RSen_P_c01_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c01_flow_direction = "Out" (IFCTEXT)
    RSen_P_c01_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c01_system_classification = "Hydronic Supply" (IFCTEXT)
    RSen_P_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c02_description = "c02_water in conection" (IFCTEXT)
    RSen_P_c02_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c02_flow_direction = "In" (IFCTEXT)
    RSen_P_c02_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c02_system_classification = "Hydronic Return" (IFCTEXT)
    RSen_P_c02_yes_no = TRUE (IFCBOOLEAN)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Family Name = "RSen_55_GM_FB_logo outdoor unit - SH_daikin" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "Daikin Europe N.V." (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "eblq011cav3 - altherma monobloc_daikin_eblq" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_alignment = "Center" (IFCTEXT)
    RSen_C_alignment_index = 0 (IFCINTEGER)
    RSen_C_component_02_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_03_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_04_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_mounting = "On the floor" (IFCTEXT)
    RSen_C_mounting_index = 0 (IFCINTEGER)
    RSen_C_offset_from_base_level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_offset_from_wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_placement = "Spacing Default" (IFCTEXT)
    RSen_C_placement_index = 0 (IFCINTEGER)
    TBQen_C_GOg = TRUE (IFCBOOLEAN)
    TBQen_C_SOg = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RSen_C_diameter_type = "OD" (IFCTEXT)
    RSen_C_diameter_type_index = 1 (IFCINTEGER)
    TBQen_C_SOg_01 = "standard" (IFCLABEL)
    TBQen_C_SOg_02 = "standard" (IFCLABEL)
    TBQen_C_SOg_03 = "standard" (IFCLABEL)
    TBQen_C_SOg_04 = "standard" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 41.4335833219003 (IFCAREAMEASURE) [SQUARE_METRE]
    RSen_C_height = 1348. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 1156. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 351. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 9.29830559507149 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.0357721843602404 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 6.71532731003365E-5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    TBQ_I Spacing_default = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQ_I Spacing_minimum = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    RSen_E_c01_apparent_power_phase_1 = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 0. (IFCPOWERMEASURE) [WATT]
  Graphics | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_clearance_zone = FALSE (IFCBOOLEAN)
    RSen_C_connection_zone = FALSE (IFCBOOLEAN)
    RSen_C_maintenance_zone = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit_displacement_back = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_front = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_logo = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "56.10.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Heat Pump" (IFCTEXT)
    Manufacturer = "Daikin Europe N.V." (IFCTEXT)
    Model = "Altherma Monobloc" (IFCTEXT)
    OmniClass Number = "23.75.10.21.14" (IFCTEXT)
    OmniClass Title = "Rooftop Heat Pumps" (IFCTEXT)
    RSen_C_IFC_version = "2x3" (IFCTEXT)
    RSen_C_code_ETIM = "" (IFCTEXT)
    RSen_C_code_ETIM_URL = "" (IFCTEXT)
    RSen_C_code_article = "EBLQ011CAV3" (IFCTEXT)
    RSen_C_code_gtin = "" (IFCTEXT)
    RSen_C_code_product = "EBLQ011CV3" (IFCTEXT)
    RSen_C_code_product_class = "EBLQ" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "31/07/2018" (IFCTEXT)
    RSen_C_content_date_issue = "31/07/2018" (IFCTEXT)
    RSen_C_content_provider = "Daikin Europe N.V." (IFCTEXT)
    RSen_C_content_version = "1.1.0" (IFCTEXT)
    RSen_C_data_issue_date = "" (IFCTEXT)
    RSen_C_description = "Heat Pump" (IFCTEXT)
    RSen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    RSen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    RSen_C_model = "Altherma Monobloc" (IFCTEXT)
    RSen_C_revit_version = "2016" (IFCTEXT)
    RSen_C_type = "Heating" (IFCTEXT)
    RSen_C_type_comments = "Outdoor unit" (IFCTEXT)
    TBQ_I BaseKeynote = "56.10.10" (IFCTEXT)
    Type Comments = "Outdoor unit" (IFCTEXT)
    Type Name = "eblq011cav3 - altherma monobloc_daikin_eblq" (IFCTEXT)
    URL = "www.daikineurope.com" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standard" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_P_c01_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c02_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Supply,Hydronic Return,Power,Controls" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_content_manual = "http://www.witas.be/en/daikin" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "standard" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_division_engine = FALSE (IFCBOOLEAN)
    RSen_E_c01_load_class = "Other" (IFCLABEL)
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_power_factor = 1. (IFCREAL)
    RSen_E_c01_voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 202 196 176 T00 silk gray_gen" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 000 163 228 T00 blue_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    COP = "4.60 (1)/2.75 (3)/3.55 (2)/2.10 (4)" (IFCTEXT)
    Casing Colour = "Ivory white" (IFCTEXT)
    Current Recommended fuses A = "40 A" (IFCTEXT)
    Dimensions Unit Height/Width/Depth mm = "1348/1160/380 mm" (IFCTEXT)
    Heating capacity Max. kW = "8.60 (3)/8.60 (4) kW" (IFCTEXT)
    Heating capacity Nom. kW = "11.2 (1)/11.0 (2) kW" (IFCTEXT)
    Installation Manual = "http://www.daikineurope.com/support-and-manuals/product-information/index.jsp?searchterm=EBLQ&searchcategory=product-information" (IFCTEXT)
    Operation range Cooling Ambient Min./Max. °CDB = "10 °CDB/46 °CDB" (IFCTEXT)
    Operation range Cooling Water side Min./Max. °C = "5 °C/22 °C" (IFCTEXT)
    Operation range Domestic hot water Ambient Min./Max. °CDB = "-25 °CDB/35 °CDB" (IFCTEXT)
    Operation range Domestic hot water Water side Min./Max. °C = "25 °C/80 °C" (IFCTEXT)
    Operation range Heating Ambient Min./Max. °CWB = "-10 °CWB/35 °CWB" (IFCTEXT)
    Operation range Heating Water side Min./Max. °C = "-15 °C/55 °C" (IFCTEXT)
    Piping connections High and low pressure gas OD mm = "-" (IFCTEXT)
    Piping connections Liquid OD mm = "-" (IFCTEXT)
    Piping connections Suction OD mm = "-" (IFCTEXT)
    Power input Heating Nom. kW = "2.43 (1)/3.10 (2) kW" (IFCTEXT)
    Power supply Phase/Frequency Hz/Voltage V = "1~/50 Hz/230 V" (IFCTEXT)
    Refrigerant Charge kg = "3.40 kg" (IFCTEXT)
    Refrigerant Type = "R-410A" (IFCTEXT)
    Sound power level Cooling Nom. dBA = "64 dBA" (IFCTEXT)
    Sound power level Heating Nom. dBA = "64 dBA" (IFCTEXT)
    Sound pressure level Cooling Nom. dBA = "50 dBA" (IFCTEXT)
    Sound pressure level Heating Nom. dBA = "51 dBA" (IFCTEXT)
    Sound pressure level Night quiet mode Cooling dBA = "45 dBA" (IFCTEXT)
    Sound pressure level Night quiet mode Heating dBA = "42 dBA" (IFCTEXT)
    Specification Text = "https://my.daikin.eu/denv/en_US/home/applications/asset-finder.html##%3Fi=1%3Bq4=document-language%253Aen%7Cdocument-language%253Anone%3Bq5=document-type%253Aspecification-text%3Bsort=date%3Bsp_d=specific%3Bsp_start_day=1%3Bsp_start_month=1%3Bsp_start_year=2011%3Btemplate=json%3Bx3=market%3Bx4=document-language%3Bx5=document-type%3Bq=EBLQ%3B" (IFCTEXT)
    Water circuit Piping connections diameter inch = "G 1"1/4 (female) inch" (IFCTEXT)
    Weight Unit kg = "151 kg" (IFCTEXT)