IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2019-04-10T08:06:04"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20181011_1500(x64) - Exporter 18.4.0.0 - ARCHICAD Connection 21.0.0.6007"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "e.suszcz" of Organization (no name given)
  Owner history of Person "e.suszcz" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "ewaq008bavp - chiller_daikin_ewaq-bvp" | object type "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin:ewaq008bavp - chiller_daikin_ewaq-bvp" | names: "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin:ewaq008bavp - chiller_daikin_ewaq-bvp:451816" | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCUNITARYEQUIPMENTTYPE "ewaq008bavp - chiller_daikin_ewaq-bvp" | ROOFTOPUNIT | 1 occurrence | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Constraints, Construction, Dimensions, Electrical, Electrical - Loads, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin:ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "Daikin Europe N.V." (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin:ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Reference Plane : h_leftright" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_alignment = "Center" (IFCTEXT)
    RSen_C_alignment_index = 0 (IFCINTEGER)
    RSen_C_component_02_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_03_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_04_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_offset_from_base_level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_placement = "Spacing Default" (IFCTEXT)
    RSen_C_placement_index = 0 (IFCINTEGER)
    TBQen_C_GOg = FALSE (IFCBOOLEAN)
    TBQen_C_SOg = TRUE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RSen_C_diameter_type = "DN" (IFCTEXT)
    RSen_C_diameter_type_index = 0 (IFCINTEGER)
    TBQen_C_SOg_01 = "standard" (IFCLABEL)
    TBQen_C_SOg_02 = "standard" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 32.4816089570934 (IFCAREAMEASURE) [SQUARE_METRE]
    RSen_C_height = 997. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 1156. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 352. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 6.89677606939294 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    TBQ_I Spacing_default = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQ_I Spacing_minimum = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    RSen_E_c01_apparent_power_phase_1 = 1525.66666666667 (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 1525.66666666667 (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 1525.66666666667 (IFCPOWERMEASURE) [WATT]
  Graphics | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_clearance_zone = FALSE (IFCBOOLEAN)
    RSen_C_connection_zone = FALSE (IFCBOOLEAN)
    RSen_C_maintenance_zone = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit_displacement_back = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_front = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_logo = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "79" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "55.10.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "chiller" (IFCTEXT)
    Manufacturer = "Daikin Europe N.V." (IFCTEXT)
    Model = "Cooling Only" (IFCTEXT)
    OmniClass Number = "23.75.10.21.14" (IFCTEXT)
    OmniClass Title = "Rooftop Heat Pumps" (IFCTEXT)
    RSen_C_IFC_version = "2x3" (IFCTEXT)
    RSen_C_code_ETIM = "Airco splitsysteem - multi split condensingunit luchtgekoeld" (IFCTEXT)
    RSen_C_code_ETIM_URL = "https://prod.etim-international.com/Class/Details?classId=EC011584&classVersion=2" (IFCTEXT)
    RSen_C_code_article = "EWAQ008BAVP" (IFCTEXT)
    RSen_C_code_gtin = "" (IFCTEXT)
    RSen_C_code_product = "EWAQ008BVP" (IFCTEXT)
    RSen_C_code_product_class = "EWAQ-BVP" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "30/04/2019" (IFCTEXT)
    RSen_C_content_date_issue = "30/04/2019" (IFCTEXT)
    RSen_C_content_provider = "Daikin Europe N.V." (IFCTEXT)
    RSen_C_content_version = "1.1.1" (IFCTEXT)
    RSen_C_data_issue_date = "" (IFCTEXT)
    RSen_C_description = "chiller" (IFCTEXT)
    RSen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    RSen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    RSen_C_model = "Cooling Only" (IFCTEXT)
    RSen_C_revit_version = "2016" (IFCTEXT)
    RSen_C_type = "Air cooled mini inverter chiller" (IFCTEXT)
    RSen_C_type_comments = "Single Unit" (IFCTEXT)
    TBQ_I BaseKeynote = "55.10.10" (IFCTEXT)
    Type Comments = "Single Unit" (IFCTEXT)
    Type Name = "ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCTEXT)
    URL = "www.daikineurope.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_P_c01_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c02_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Return,Power,Hydronic Supply,Communication" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCLABEL)
    Family and Type = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCLABEL)
    Type = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCLABEL)
    Type Id = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq008bavp - chiller_daikin_ewaq-bvp" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin" (IFCTEXT)
    RSen_E_c01_description = "c01_el" (IFCTEXT)
    RSen_E_c01_power_factor_state = "Lagging" (IFCTEXT)
    RSen_E_c01_system_type = "Power - Unbalanced" (IFCTEXT)
    RSen_E_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_E_c02_description = "c02_controls" (IFCTEXT)
    RSen_E_c02_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c01_description = "c01_chilled water in connection" (IFCTEXT)
    RSen_P_c01_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c01_flow_direction = "In" (IFCTEXT)
    RSen_P_c01_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c01_system_classification = "Hydronic Return" (IFCTEXT)
    RSen_P_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c02_description = "c02_chilled water out connection" (IFCTEXT)
    RSen_P_c02_diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter_calc = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_flow_configuration = "Preset" (IFCTEXT)
    RSen_P_c02_flow_direction = "Out" (IFCTEXT)
    RSen_P_c02_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c02_system_classification = "Hydronic Supply" (IFCTEXT)
    RSen_P_c02_yes_no = TRUE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_content_manual = "http://www.witas.be/en/daikin" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 4577. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 19.9 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_division_engine = FALSE (IFCBOOLEAN)
    RSen_E_c01_load_class = "Other" (IFCLABEL)
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_power = 2570. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_power_factor = 1. (IFCREAL)
    RSen_E_c01_voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 202 196 176 T00 silk gray_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Air heat exchanger Type = "Cross fin coil/Hi-X tubes and PE coated waffle louvre fins" (IFCTEXT)
    Capacity control Method = "Variable (inverter)" (IFCTEXT)
    Capacity control Minimum capacity % = "-" (IFCTEXT)
    Compressor Quantity = "1" (IFCTEXT)
    Compressor Type = "Hermetically sealed swing compressor" (IFCTEXT)
    Cooling capacity Nom. kW = "7,95 (1)/8,23 (2) kW" (IFCTEXT)
    Dimensions Unit Depth mm = "380 mm" (IFCTEXT)
    Dimensions Unit Height mm = "997 mm" (IFCTEXT)
    Dimensions Unit Width mm = "1160 mm" (IFCTEXT)
    EER kW = "3,10 (1)/4,99 (2)" (IFCTEXT)
    ESEER = "5,24 (5)" (IFCTEXT)
    Fan Air flow rate Cooling Nom. m3/min = "72 (1) m³/min" (IFCTEXT)
    Fan Quantity = "1" (IFCTEXT)
    Fan Type = "Propeller fan" (IFCTEXT)
    Installation Manual = "http://www.daikineurope.com/support-and-manuals/product-information/index.jsp?searchterm=EWAQ-BVP&searchcategory=product-information" (IFCTEXT)
    Operation range Air side Cooling Min./Max. °CDB = "10 °CDB/46 °CDB" (IFCTEXT)
    Operation range Water side Cooling Min./Max. °CDB = "5 °CDB/22 °CDB" (IFCTEXT)
    Power input Cooling Nom. kW = "2,57 (1)/1,65 (2) kW" (IFCTEXT)
    Power supply Phase/Frequency Hz/Voltage V = "1N~/50/230 V" (IFCTEXT)
    Refrigerant Circuits Quantity = "1" (IFCTEXT)
    Refrigerant Control = "Electronic expansion valve" (IFCTEXT)
    Refrigerant Type/GWP = "R-410A /2,087,5" (IFCTEXT)
    Refrigerant charge Per circuit TCO2Eq = "5,6 TCO2Eq" (IFCTEXT)
    Refrigerant charge Per circuit kg = "2,70 kg" (IFCTEXT)
    Sound power level Cooling Nom. dBA = "69 (1) dBA" (IFCTEXT)
    Specification Text = "https://my.daikin.eu/denv/en_US/home/applications/asset-finder.html##%3Fi=1%3Bq4=document-language%253Aen%7Cdocument-language%253Anone%3Bq5=document-type%253Aspecification-text%3Bsort=date%3Bsp_d=specific%3Bsp_start_day=1%3Bsp_start_month=1%3Bsp_start_year=2011%3Btemplate=json%3Bx3=market%3Bx4=document-language%3Bx5=document-type%3Bq=EWAQ-BVP%3B" (IFCTEXT)
    Unit Running current Max A = "19,9 A" (IFCTEXT)
    Unit Starting current Max A = "19,9 (12) A" (IFCTEXT)
    Water circuit Piping connections diameter inch = "1" MBSP inch" (IFCTEXT)
    Water circuit Piping inch = "-" (IFCTEXT)
    Water heat exchanger Type = "Brazed plate" (IFCTEXT)
    Water heat exchanger Water flow rate Cooling Nom. l/min = "22,8 (1)/23,6 (2) l/min" (IFCTEXT)
    Water heat exchanger Water pressure drop Cooling Total kPa = "-" (IFCTEXT)
    Water heat exchanger Water volume l = "2 l" (IFCTEXT)
    Weight Operation weight kg = "-" (IFCTEXT)
    Weight Unit kg = "106 kg" (IFCTEXT)

Other addresses and roles
  2 x postal address: "## Street City, State Zip", "Boston", "MA"