IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2018-10-17T14:32:30"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20161004_0715(x64) - Exporter 16.0.1185.0 - Default UI"
Application: "Autodesk Revit MEP 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit MEP 2016 (ENU)"

People and organizations
  Person "e.suszcz" of Organization (no name given)
  Owner history of Person "e.suszcz" of Organization (no name given) | application "Autodesk Revit MEP 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit MEP 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "X:\ZZ\01\RSen_55_ME_FB_air cooled chiller (cooling only)_daikin_ifc\RSen_55_ME_FB_air cooled chiller (cooling only)_daikin_ewaq021cawn - inverter_daikin_ewaq-cwn.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "ewaq021cawn - inverter_daikin_ewaq-cwn" | object type "ewaq021cawn - inverter_daikin_ewaq-cwn" | names: "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin:ewaq021cawn - inverter_daikin_ewaq-cwn:5152498" | material: materials ("RSen_x_rgb 189 187 185 T80 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Construction, Dimensions, Electrical - Loads
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standard" | object type "standard" | names: "RSen_55_GM_FB_logo outdoor unit - SH_daikin:standard:5152499" | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen") | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing

Types
  IFCUNITARYEQUIPMENTTYPE "ewaq021cawn - inverter_daikin_ewaq-cwn" | ROOFTOPUNIT | 1 occurrence | material: materials ("RSen_x_rgb 189 187 185 T80 gray_gen", "RSen_x_rgb 202 196 176 T00 silk gray_gen") | property sets: Constraints, Construction, Dimensions, Electrical, Electrical - Loads, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "standard" | 1 occurrence | material: materials ("RSen_x_rgb 000 163 228 T00 blue_gen", "RSen_x_rgb 079 201 245 T00 blue_gen", "RSen_x_rgb 055 053 053 T00 gray_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCLABEL)
    Family and Type = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
    Type = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCLABEL)
    Type Id = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin: ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Family and Type = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Type = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
    Type Id = "RSen_55_GM_FB_logo outdoor unit - SH_daikin: standard" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "RSen_55_ME_FB_air cooled chiller (cooling only)_daikin" (IFCTEXT)
    RSen_E_c01_description = "c01_el" (IFCTEXT)
    RSen_E_c01_power_factor_state = "Lagging" (IFCTEXT)
    RSen_E_c01_system_type = "Power - Unbalanced" (IFCTEXT)
    RSen_E_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_E_c02_description = "c02_controls" (IFCTEXT)
    RSen_E_c02_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c01_description = "c01_chilled water in connection" (IFCTEXT)
    RSen_P_c01_diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_diameter_calc = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_flow_configuration = "Calculated" (IFCTEXT)
    RSen_P_c01_flow_direction = "In" (IFCTEXT)
    RSen_P_c01_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c01_system_classification = "Hydronic Return" (IFCTEXT)
    RSen_P_c01_yes_no = TRUE (IFCBOOLEAN)
    RSen_P_c02_description = "c02_chilled water out connection" (IFCTEXT)
    RSen_P_c02_diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_diameter_calc = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c02_flow_configuration = "Preset" (IFCTEXT)
    RSen_P_c02_flow_direction = "Out" (IFCTEXT)
    RSen_P_c02_loss_method = "Not Defined" (IFCTEXT)
    RSen_P_c02_system_classification = "Hydronic Supply" (IFCTEXT)
    RSen_P_c02_yes_no = TRUE (IFCBOOLEAN)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Family Name = "RSen_55_GM_FB_logo outdoor unit - SH_daikin" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "Daikin Europe N.V." (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 type object
    Default Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_alignment = "Center" (IFCTEXT)
    RSen_C_alignment_index = 0 (IFCINTEGER)
    RSen_C_component_02_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_03_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_component_04_offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_offset_from_base_level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_placement = "Spacing Default" (IFCTEXT)
    RSen_C_placement_index = 0 (IFCINTEGER)
    TBQen_C_GOg = TRUE (IFCBOOLEAN)
    TBQen_C_SOg = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RSen_C_diameter_type = "DN" (IFCTEXT)
    RSen_C_diameter_type_index = 0 (IFCINTEGER)
    TBQen_C_SOg_01 = "standard" (IFCLABEL)
    TBQen_C_SOg_02 = "standard" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 72.7865790715782 (IFCAREAMEASURE) [SQUARE_METRE]
    RSen_C_height = 1684. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 1371. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 774. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 27.7142287786667 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.0357721843602404 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 6.71532731003365E-5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    TBQ_I Spacing_default = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQ_I Spacing_minimum = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    RSen_E_c01_apparent_power_phase_1 = 3373.33333333333 (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_2 = 3373.33333333333 (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_apparent_power_phase_3 = 3373.33333333333 (IFCPOWERMEASURE) [WATT]
  Graphics | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_clearance_zone = FALSE (IFCBOOLEAN)
    RSen_C_connection_zone = FALSE (IFCBOOLEAN)
    RSen_C_maintenance_zone = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit = FALSE (IFCBOOLEAN)
    RSen_C_neighbour_unit_displacement_back = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_front = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_neighbour_unit_displacement_right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_logo = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "9" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "55.10.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Cooling Only" (IFCTEXT)
    Manufacturer = "Daikin Europe N.V." (IFCTEXT)
    Model = "Inverter" (IFCTEXT)
    OmniClass Number = "23.75.10.21.14" (IFCTEXT)
    OmniClass Title = "Rooftop Heat Pumps" (IFCTEXT)
    RSen_C_IFC_version = "2x3" (IFCTEXT)
    RSen_C_code_ETIM = "Airco splitsysteem - multi split condensingunit luchtgekoeld" (IFCTEXT)
    RSen_C_code_ETIM_URL = "https://prod.etim-international.com/Class/Details?classId=EC011584&classVersion=2" (IFCTEXT)
    RSen_C_code_article = "EWAQ021CAWN" (IFCTEXT)
    RSen_C_code_gtin = "" (IFCTEXT)
    RSen_C_code_product = "EWAQ021CAWN" (IFCTEXT)
    RSen_C_code_product_class = "EWAQ-CWN" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "31/05/2018" (IFCTEXT)
    RSen_C_content_date_issue = "31/05/2018" (IFCTEXT)
    RSen_C_content_provider = "Daikin Europe N.V." (IFCTEXT)
    RSen_C_content_version = "1.1.0" (IFCTEXT)
    RSen_C_data_issue_date = "" (IFCTEXT)
    RSen_C_description = "Cooling Only" (IFCTEXT)
    RSen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    RSen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    RSen_C_model = "Inverter" (IFCTEXT)
    RSen_C_revit_version = "2016" (IFCTEXT)
    RSen_C_type = "Air cooled scroll inverter chiller" (IFCTEXT)
    RSen_C_type_comments = "Single Unit" (IFCTEXT)
    TBQ_I BaseKeynote = "55.10.10" (IFCTEXT)
    Type Comments = "Single Unit" (IFCTEXT)
    Type Name = "ewaq021cawn - inverter_daikin_ewaq-cwn" (IFCTEXT)
    URL = "www.daikineurope.com" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standard" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_P_c01_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    RSen_P_c02_volume_flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Return,Power,Hydronic Supply,Communication" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    RSen_C_content_manual = "http://www.witas.be/en/daikin" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "standard" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 10120. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 25.3 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_division_engine = FALSE (IFCBOOLEAN)
    RSen_E_c01_load_class = "Other" (IFCLABEL)
    RSen_E_c01_number_of_poles = 3 (IFCINTEGER)
    RSen_E_c01_power = 7610. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_power_factor = 1. (IFCREAL)
    RSen_E_c01_voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 202 196 176 T00 silk gray_gen" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_x_rgb 000 163 228 T00 blue_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Air heat exchanger Type = "Air cooled coil" (IFCTEXT)
    Capacity control Method = "Inverter controlled" (IFCTEXT)
    Capacity control Minimum capacity % = "25%" (IFCTEXT)
    Compressor Quantity = "2" (IFCTEXT)
    Compressor Type = "Hermetically sealed scroll compressor" (IFCTEXT)
    Cooling capacity Nom. kW = "21,0 (1) kW" (IFCTEXT)
    Dimensions Unit Depth mm = "774 mm" (IFCTEXT)
    Dimensions Unit Height mm = "1,684 mm" (IFCTEXT)
    Dimensions Unit Width mm = "1,370 mm" (IFCTEXT)
    EER kW = "2,77" (IFCTEXT)
    ESEER = "4,26" (IFCTEXT)
    Fan Air flow rate Cooling Nom. m3/min = "185 m³/min" (IFCTEXT)
    Fan Quantity = "1" (IFCTEXT)
    Fan Type = "Axial" (IFCTEXT)
    Installation Manual = "http://www.daikineurope.com/support-and-manuals/product-information/index.jsp?searchterm=EWAQ-CWN&searchcategory=product-information" (IFCTEXT)
    Operation range Air side Cooling Min./Max. °CDB = "-5 °CDB/43 °CDB" (IFCTEXT)
    Operation range Water side Cooling Min./Max. °CDB = "-10 °CDB/20 °CDB" (IFCTEXT)
    Power input Cooling Nom. kW = "7,61 (1) kW" (IFCTEXT)
    Power supply Phase/Frequency Hz/Voltage V = "3N~ /50 Hz/400 V" (IFCTEXT)
    Refrigerant Circuits Quantity = "1" (IFCTEXT)
    Refrigerant Control = "Electronic expansion valve" (IFCTEXT)
    Refrigerant Type/GWP = "R-410A /2,087,5" (IFCTEXT)
    Refrigerant charge Per circuit TCO2Eq = "15,9 TCO2Eq" (IFCTEXT)
    Refrigerant charge Per circuit kg = "7,60 kg" (IFCTEXT)
    Sound power level Cooling Nom. dBA = "78 dBA" (IFCTEXT)
    Specification Text = "https://my.daikin.eu/denv/en_US/home/applications/asset-finder.html##%3Fi=1%3Bq4=document-language%253Aen%7Cdocument-language%253Anone%3Bq5=document-type%253Aspecification-text%3Bsort=date%3Bsp_d=specific%3Bsp_start_day=1%3Bsp_start_month=1%3Bsp_start_year=2011%3Btemplate=json%3Bx3=market%3Bx4=document-language%3Bx5=document-type%3Bq=EWAQ-CWN%3B" (IFCTEXT)
    Unit Running current Max A = "25,3 A" (IFCTEXT)
    Unit Starting current Max A = "77,7 A" (IFCTEXT)
    Water circuit Piping connections diameter inch = "1-1/4" (female) inch" (IFCTEXT)
    Water circuit Piping inch = "1-1/4" inch" (IFCTEXT)
    Water heat exchanger Type = "Brazed plate" (IFCTEXT)
    Water heat exchanger Water flow rate Cooling Nom. l/min = "60 (2) l/min" (IFCTEXT)
    Water heat exchanger Water pressure drop Cooling Total kPa = "10 kPa" (IFCTEXT)
    Water heat exchanger Water volume l = "3 l" (IFCTEXT)
    Weight Operation weight kg = "-" (IFCTEXT)
    Weight Unit kg = "321 kg" (IFCTEXT)