IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2022-05-25T10:24:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.0.0.383 - Exporter 21.2.1.0 - Alternate UI 21.2.1.0"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "info" of Organization (no name given)
  Owner history of Person "info" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1653466915 (2022-05-25T08:21:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:347660" | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI" | object type "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI" | names: "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI:347668" | material: materials ("Latón, pintado blanco", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCWALLTYPE "Basic Wall:Generic - 200mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBOILERTYPE "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI" | 1 occurrence | material: "Latón, pintado blanco" | property sets: Constraints, Data, Dimensions, General, Green Building Properties, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Generic - 200mm" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Ano Produccion = "" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Autor = "De Dietrich Thermique Iberia, S.L.U." (IFCTEXT)
    Base Precio Producto 01 = "" (IFCTEXT)
    Base Precio Producto 02 = "" (IFCTEXT)
    Base Precio Producto 03 = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Codigo = "INIDENS 24" (IFCTEXT)
    Condiciones de Venta = "" (IFCTEXT)
    Description = "Calderas murales de condensación de gas completamente preajustadas, equipadas para funcionar con gas natural o propano." (IFCTEXT)
    Email Contacto = "info@dedietrichthemique.es" (IFCTEXT)
    Etiqueta Modelo = "INIDENS 24" (IFCTEXT)
    Fecha Emision Elemento BIM = "25.05.2022" (IFCTEXT)
    Fecha Vencimiento Elemento BIM = "25.05.2023" (IFCTEXT)
    Historial = "(RVT2021) Creación de Elemento." (IFCTEXT)
    Informacion Tecnica = "https://www.dedietrich-calefaccion.es/download/file?file=var/ddth/storage/original/application/f0647964f0aa059b114d64cc7919898b.pdf&filename=Folleto_te_cnico_INIDENS_20_05.pdf" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique Iberia, S.L.U." (IFCTEXT)
    Marcado CE = FALSE (IFCBOOLEAN)
    Model = "INIDENS 24" (IFCTEXT)
    Numero Articulo = "" (IFCTEXT)
    Numero Articulo Global Comercial = "" (IFCTEXT)
    Numero de Declaracion de Prestaciones = "" (IFCTEXT)
    Numero de Licencia = "XXX-XXXX7125" (IFCTEXT)
    OmniClass Number = "23.65.35.11" (IFCTEXT)
    OmniClass Title = "Supply Water Heaters" (IFCTEXT)
    Pais de Venta = "" (IFCTEXT)
    Partida URL = "" (IFCTEXT)
    Plataforma descaga contenido BIM = "www.bimetica.com" (IFCTEXT)
    Referencia = "INIDENS" (IFCTEXT)
    Referencia Contacto Comercial Venta = "" (IFCTEXT)
    Referencia Contacto Soporte Tecnico = "" (IFCTEXT)
    Serie = "INIDENS" (IFCTEXT)
    Soporte tecnico BIM = "https://bimsupport.info/es/fabricantes/de-dietrich-bim/" (IFCTEXT)
    Telefono Contacto = "+34 900 802 143" (IFCTEXT)
    Titular = "De Dietrich Thermique Iberia, S.L.U." (IFCTEXT)
    Type Name = "INIDENS 30/35 MI" (IFCTEXT)
    URL = "www.dedietrich-calefaccion.es" (IFCTEXT)
    URL Perfil BIM = "https://bimetica.com/es/objeto-bim-dedietrich-caldera-gas-inidens-11066.html" (IFCTEXT)
    URL Producto = "https://www.dedietrich-calefaccion.es/productos/gama_de_productos/calderas_murales_domesticas/gas_de_condensacion_inidens" (IFCTEXT)
    URL de Declaracion de Prestaciones = "" (IFCTEXT)
    Unidad Medicion = "Unidad" (IFCTEXT)
    Version = "RVT2021" (IFCTEXT)
    Version Estandar GDO-BIM = "GDO-BIM V02" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Family and Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "2021_ES_Caldera_De-Dietrich_Inidens: INIDENS 30/35 MI" (IFCLABEL)
    Family and Type = "2021_ES_Caldera_De-Dietrich_Inidens: INIDENS 30/35 MI" (IFCLABEL)
    Host Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "2021_ES_Caldera_De-Dietrich_Inidens: INIDENS 30/35 MI" (IFCLABEL)
    Type Id = "2021_ES_Caldera_De-Dietrich_Inidens: INIDENS 30/35 MI" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Walls" (IFCLABEL)
    Family Name = "Basic Wall" (IFCTEXT)
  Other | properties | on 1 type object
    Altura minima requerida = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Dependiente De = "" (IFCTEXT)
    Es Accesible = TRUE (IFCBOOLEAN)
    Espacio libre acceso = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Estandar seguridad = "" (IFCTEXT)
    Family Name = "2021_ES_Caldera_De-Dietrich_Inidens" (IFCTEXT)
    Nivel de Riesgo = "" (IFCTEXT)
    Responsable Seguridad = "" (IFCTEXT)
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.2 [SQUARE_METRE]
    GrossSideArea = 2. [SQUARE_METRE]
    GrossVolume = 0.4 [CUBIC_METRE]
    Height = 2000. [MILLI METRE]
    Length = 1000. [MILLI METRE]
    NetSideArea = 2. [SQUARE_METRE]
    NetVolume = 0.4 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Elevation from Level = 1199. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Desfase = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 2. (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Area = 0.640254999999991 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0873581999999978 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Altura = 776. (IFCLENGTHMEASURE) [MILLI METRE]
    Anchura = 395. (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Desagüe Válvula Seguridad = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Desagüe de Condensados = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Entrada Agua Fría = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Impulsión Calefacción = 19.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Retorno Calefacción = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Salida ACS = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Salida Gases Combustión = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Profundidad = 285. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 2 objects (1 IFCENERGYCONVERSIONDEVICE, 1 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Codigo Barras = "" (IFCTEXT)
    Fecha Colocacion = "" (IFCTEXT)
    Fecha Compra = "" (IFCTEXT)
    Fecha Suministro = "" (IFCTEXT)
    Instrucciones Especiales = "" (IFCTEXT)
    Lugar Ensamblaje = "" (IFCTEXT)
    Material Contenedor = "" (IFCTEXT)
    Material Envoltura = "" (IFCTEXT)
    Numero Serie = "" (IFCTEXT)
    Referencia Lote = "" (IFCTEXT)
    Responsable Compra = "" (IFCTEXT)
    Tipo Embalaje Proteccion = "" (IFCTEXT)
  Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "Basic Wall:Generic - 200mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "Basic Wall:Generic - 200mm" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Generic - 200mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Reference = "2021_ES_Caldera_De-Dietrich_Inidens:INIDENS 30/35 MI" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE) | on 1 type object
    Manufacturer = "De Dietrich Thermique Iberia, S.L.U." (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Hydronic Return,Domestic Hot Water,Other,Domestic Cold Water,Domestic Hot Water,Exhaust Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Caudal ACS = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Classification = "None" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Data | properties | on 1 type object
    Calificacion de presion = 100. (IFCPRESSUREMEASURE) [PASCAL]
    Capacidad de almacenamiento de agua = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Consumo nominal de energia = 30000. (IFCPOWERMEASURE) [WATT]
    Curvas de eficiencia de carga parcial = 0. (IFCREAL)
    Es Exterior = FALSE (IFCBOOLEAN)
    Es calentador de almacenamiento de agua = TRUE (IFCBOOLEAN)
    Espacio = "" (IFCTEXT)
    Fuente de energia = "gas natural o propano" (IFCTEXT)
    Modo operativo = "" (IFCTEXT)
    Rango de temperatura de salida = "de 25 a 80 °C" (IFCTEXT)
    Rango de temperatura de suministro de agua = "de 35 a 60 °C" (IFCTEXT)
    Relacion de carga parcial nominal = 0. (IFCREAL)
    Responsable Prescripcion = "" (IFCTEXT)
    Sistema = "" (IFCTEXT)
    Zona = "" (IFCTEXT)
    Área de Superficie de Transferencia de Calor = 0. (IFCAREAMEASURE) [SQUARE_METRE]
  General | properties | on 1 type object
    Condiciones Evaluacion = "" (IFCTEXT)
    Contacto = "" (IFCTEXT)
    Contenido Garantia = "" (IFCTEXT)
    Coste Mantenimiento = 0. (IFCREAL)
    Descripcion Evaluacion = "" (IFCTEXT)
    Exclusiones = "" (IFCTEXT)
    Fecha Evaluacion = "" (IFCTEXT)
    Fecha Fin Garantia = "" (IFCTEXT)
    Fecha Inicio Garantia = "" (IFCTEXT)
    Garantia Extendida = TRUE (IFCBOOLEAN)
    Identificador Garantia = "" (IFCTEXT)
    Mantenimiento = "" (IFCTEXT)
    Periodo Garantia = "" (IFCTEXT)
    Punto de Contacto = "" (IFCTEXT)
    Tiempo Medio Entre Fallos = "" (IFCTEXT)
    Tiempo Util De Vida = "" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Acidificacion Atmosferica por Unidad = 0. (IFCREAL)
    Agua Consumida por Unidad = 0. (IFCREAL)
    Cambio Climatico por Unidad = 0. (IFCREAL)
    Creditos BREEAM = "" (IFCTEXT)
    Creditos LEED = "" (IFCTEXT)
    Declaracion Ambiental de Producto URL = "" (IFCTEXT)
    Destruccion Capa Ozono Estratosferica por Unidad = 0. (IFCREAL)
    Energia No Renovable Consumida por Unidad = 0. (IFCREAL)
    Energia Primaria Total Consumida por Unidad = 0. (IFCREAL)
    Energia Renovable Consumida por Unidad = 0. (IFCREAL)
    Energia consumida = 0. (IFCREAL)
    Eutrofizacion por Unidad = 0. (IFCREAL)
    Falta de Recursos por Unidad = 0. (IFCREAL)
    Fase Ciclo Vida = "" (IFCTEXT)
    Formacion Fotoquimica Ozono por Unidad = 0. (IFCREAL)
    Fuente Datos LCA = "" (IFCTEXT)
    Referencia Unidad Funcional = "" (IFCTEXT)
    Residuo Inerte por Unidad = 0. (IFCREAL)
    Residuo Radioactivo por Unidad = 0. (IFCREAL)
    Residuos No Peligrosos por Unidad = 0. (IFCREAL)
    Residuos Peligrosos por Unidad = 0. (IFCREAL)
    Unidad = "" (IFCTEXT)
    Vida Util Esperada = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Acabado = "" (IFCTEXT)
    Material = "Latón, pintado blanco" (IFCLABEL)