IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2023-04-07T09:32:40"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "radu_orza" of Organization (no name given)
  Owner history of Person "radu_orza" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680848930 (2023-04-07T06:28:50Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "F00" | long name "F00" | object type "Level:Floor Level" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "170" | object type "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN:170" | names: "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN:170:1311380" | material: constituents "MaterialConstituentSet" ("Color RGB 176-176-176": "Color RGB 176-176-176", "Color RGB 176-000-000": "Color RGB 176-000-000", "Color RGB 000-112-208": "Color RGB 000-112-208", "Color RGB 128-128-128": "Color RGB 128-128-128", "Color RGB 040-040-040": "Color RGB 040-040-040", "Color RGB 192-192-192": "Color RGB 192-192-192", "Color RGB 229-229-000": "Color RGB 229-229-000") | property sets: Pset_BoilerTypeCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads

Types
  IFCBOILERTYPE "170" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Color RGB 176-176-176": "Color RGB 176-176-176", "Color RGB 176-000-000": "Color RGB 176-000-000", "Color RGB 000-112-208": "Color RGB 000-112-208", "Color RGB 128-128-128": "Color RGB 128-128-128", "Color RGB 040-040-040": "Color RGB 040-040-040", "Color RGB 192-192-192": "Color RGB 192-192-192", "Color RGB 229-229-000": "Color RGB 229-229-000") | property sets: Constraints, Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_BoilerTypeCommon | properties | on 1 object (1 IFCBOILER) | on 1 type object
    Reference = "170" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBOILER) | on 1 type object
    Reference = "170" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER) | on 1 type object
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Area = 8.62928984380999 (IFCAREAMEASURE) [SQUARE_METRE]
    Gas Connector Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter 1 = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter 2 = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.5806048362814 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas diameter = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1368. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 1190. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBOILER)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "F00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "High-efficiency standing gas boiler" (IFCTEXT)
    Article Type = "170" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "23.05" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "High-efficiency standing gas boiler" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC010231" (IFCTEXT)
    Family Version = "23.05" (IFCTEXT)
    GLN = "" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    Language = "" (IFCTEXT)
    MEPcontent Class = "BOILER_CONDENSATE_FLOW" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "" (IFCTEXT)
    Manufacturer URL = "https://www.dedietrich-thermique.fr/" (IFCTEXT)
    Model = "170" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2020" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "170" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBOILER)
    System Classification = "Sanitary,Hydronic Return,Other,Undefined,Supply Air,Power,Hydronic Return,Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
    Maximum Operating Pressure = 600000. (IFCPRESSUREMEASURE) [PASCAL]
    Maximum Supply Temperature (Operating Temperature) = 90. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Maximum Supply Temperature = 110. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Minimum Operating Pressure = 80000. (IFCPRESSUREMEASURE) [PASCAL]
    Nominal Power 50-30 °C (kW) = "33 - 179" (IFCTEXT)
    Nominal Power 80-60 °C (kW) = "29 - 166" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCBOILER)
    Drain Fixture Units = 0. (IFCREAL)
    Flue Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Client Name" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Project Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN: 170" (IFCLABEL)
    Family and Type = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN: 170" (IFCLABEL)
    Type = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN: 170" (IFCLABEL)
    Type Id = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN: 170" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    B = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    B2 = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Central Heating Connectors Lenght = 31. (IFCLENGTHMEASURE) [MILLI METRE]
    Family Name = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C230 Evo_INT-EN" (IFCTEXT)
    Hydronic Return Nominal Diameter = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return and Supply Fiting Visibility = FALSE (IFCBOOLEAN)
    Hydronic Supply Nominal Diameter = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "4. Plan over 10 years" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Show Service Space = FALSE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    Front Clearance = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance = 382. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Floor Level" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Voltage = 229.999999642952 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 040-040-040" (IFCLABEL)
    Blue = "Color RGB 000-112-208" (IFCLABEL)
    Dark Grey = "Color RGB 040-040-040" (IFCLABEL)
    Grey = "Color RGB 128-128-128" (IFCLABEL)
    Light Grey = "Color RGB 176-176-176" (IFCLABEL)
    Red = "Color RGB 176-000-000" (IFCLABEL)
    White = "Color RGB 192-192-192" (IFCLABEL)
    Yellow = "Color RGB 229-229-000" (IFCLABEL)

Other addresses and roles
  2 x postal address: "Enter address here"