IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "Project Number"
Time stamp: "2020-01-20T09:53:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20180216_1515(x64) - Exporter 19.0.0.405 - Alternate UI 19.0.0.405"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "Miguel" "Angel" of Organization (no name given)
  Owner history of Person "Miguel" "Angel" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "2Â½H x 2Â½H" | object type "2Â½H x 2Â½H" | names: "2019_Valvula_Arco_Sena:2Â½H x 2Â½H:204246" | material: materials ("Jatón Europeo CW617N - Chromado", "Color Rojo") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Graphics, Identity Data

Types
  IFCVALVETYPE "2Â½H x 2Â½H" | 1 occurrence | material: materials ("Jatón Europeo CW617N - Chromado", "Color Rojo") | property sets: Dimensions, Identity Data, Materials and Finishes, Mechanical, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Vávulas Arco S.L" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "2Â½H x 2Â½H" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Maximum Size = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "64 mmø-64 mmø" (IFCTEXT)
    Volume = 0.00104578637037007 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    A = 134. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 173. (IFCLENGTHMEASURE) [MILLI METRE]
    C = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 82. (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Exterior = 82. (IFCLENGTHMEASURE) [MILLI METRE]
    Diámetro Nominal = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    E = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Radio Exterior = 41. (IFCLENGTHMEASURE) [MILLI METRE]
    Radio Nominal = 31.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Radio Tuerca = 43.05 (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Cost = 60.42 (IFCREAL)
    Description = "Válvula Sena mando palanca H-H" (IFCTEXT)
    Manufacturer = "Vávulas Arco S.L" (IFCTEXT)
    Model = "150109" (IFCTEXT)
    OmniClass Number = "23.65.55.14.21" (IFCTEXT)
    OmniClass Title = "Non-Return Valves for Liquid Services" (IFCTEXT)
    Type Name = "2Â½H x 2Â½H" (IFCTEXT)
    URL = "www.valvulasarco.com" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "64 mmø-64 mmø" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    K Coefficient = 0.35 (IFCREAL)
  Mechanical - Flow | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "2019_Valvula_Arco_Sena: 2Â½H x 2Â½H" (IFCLABEL)
    Family and Type = "2019_Valvula_Arco_Sena: 2Â½H x 2Â½H" (IFCLABEL)
    Type = "2019_Valvula_Arco_Sena: 2Â½H x 2Â½H" (IFCLABEL)
    Type Id = "2019_Valvula_Arco_Sena: 2Â½H x 2Â½H" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Ancho Símbolo = 15.0111069989303 (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Pipe Accessories" (IFCLABEL)
    Family Name = "2019_Valvula_Arco_Sena" (IFCTEXT)
    HEX = FALSE (IFCBOOLEAN)
    OCT = TRUE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 type object
    Material = "Jatón Europeo CW617N - Chromado" (IFCLABEL)